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                 Obvestilo za javnost 

- 6 -

Tehnični podatki:
	2010 Ford Kuga TDCi 


	Različica
	Kuga 140 KM TDCi FWD
6-ročni menjalnik
	Kuga 140 KM TDCi AWD
6-ročni menjalnik
	Kuga 140 KM TDCi AWD
PowerShift
6-st. avtom.
	Kuga 163 KM TDCi AWD
6-ročni menjalnik
	Kuga 163 KM TDCi AWD
PowerShift
6-st. avtom.

	Max moč (KM/kW)
	140 / 103
	140 / 103
	140 / 103
	163 / 120
	163 / 120

	Max navor (Nm)
	320
	320
	320
	340
	340

	CO2 emisija* (g/km)
	156
	159
	179
	159
	179

	

	Poraba goriva* (l/100 km)
	

	Mestna vožnja
	7.5 
	7.6 
	8.5 
	7.6 
	8.5 

	Izven-mestna vožnja
	5.0 
	5.1 
	5.8 
	5.1 
	5.8 

	Kombinirana vožnja
	5.9 
	6.0 
	6.8 
	6.0 
	6.8 

	

	Najvišja hitrost km/h 
	186 
	184 
	183 
	195 
	192 

	0—100km/h (sek)
	10.2
	10.4
	10.7
	9.6
	9.9

	50—100km/h (sek)
	8.5
	8.9
	n/a
	8.1
	n/a

	

	* Vse emisije CO2 v g/km in porabe goriva v l/100 km izvirajo iz uradnih preizkusov, ki ustrezajo priporočilom 93/116/EC.  Poraba goriva se meri v skladu z EU 80/1268/EEC in ni nujno, da odraža dejanske emisije oziroma porabo goriva pri določenem modelu.



Moč/Navor graf – Duratorq TDCi 2.0-l 163 KM 
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	Engine data – Duratorq TDCi 2.0-litre 140 PS 


	Engine type
	Turbo diesel, direct injection

	Displacement (cc)
	1997

	Bore (mm)
	85,0

	Stroke (mm)
	88,0

	Fuel type, grade
	Diesel

	Max power (ISO kW/PS)
	103 (140)

	At engine speed (rpm)
	3750

	Max torque (ISO Nm)
	320

	At engine speed (rpm)
	1750 - 2750

	Compression ratio
	16.0:1

	Cylinders
	4 in line

	Cylinder head
	Cast aluminium

	Cylinder block
	Cast iron

	Crankshaft
	Drop forged steel, eight counterweights, five main bearings

	Valves per cylinder
	4

	Valve gear
	Timing belt (crankshaft to intake) with dynamic tensioner
Intake to exhaust chain with hydraulic tensioner

	Included angle between valves
	0°

	Valve sizes (mm)
	28,2 intake,  23,1 exhaust

	Turbocharger
	Variable geometry turbocharger, pneumatically actuated with position sensor

	Camshaft 
	Forged / composite camshaft, Exhaust cam drives FIP

	Pistons
	Aluminium-silicium alloy with molybdenum-coating, three piston rings

	Connecting rods
	Steel forged, trapezoid shaped small end, split big end

	Engine management
	Ford 2nd generation common rail diesel
engine management system

	Fuel injection
	Delphi common rail multiple injection
- tubular high-pressure common-rail with fuel pressure 2000 bar,
- 2 control valves (PCV/VCV), 3 pistons + internal transfer pump
- centrally located injectors, solenoid actuated, with 8-hole micro sac:
- closed loop 'minimum injection quantity' control


	Emission controls
	Oxidation catalyst, Water cooled EGR, Standard cDPF

	Emission level
	Euro Stage 5

	
	


	Engine data – Duratorq TDCi 2.0-litre 163 PS 


	Engine type
	Turbo diesel, direct injection

	Displacement (cc)
	1997

	Bore (mm)
	85,0

	Stroke (mm)
	88,0

	Fuel type, grade
	Diesel

	Max power (ISO kW/PS)
	120 (163)

	At engine speed (rpm)
	3750

	Max torque (ISO Nm)
	340

	At engine speed (rpm)
	2000 - 3250

	Compression ratio
	16.0:1

	Cylinders
	4 in line

	Cylinder head
	Cast aluminium

	Cylinder block
	Cast iron

	Crankshaft
	Drop forged steel, eight counterweights, five main bearings

	Valves per cylinder
	4

	Valve gear
	Timing belt (crankshaft to intake) with dynamic tensioner
Intake to exhaust chain with hydraulic tensioner

	Included angle between valves
	0°

	Valve sizes (mm)
	28,2 intake,  23,1 exhaust

	Turbocharger
	Variable geometry turbocharger, pneumatically actuated with position sensor

	Camshaft 
	Forged / composite camshaft, Exhaust cam drives FIP

	Pistons
	Aluminium-silicium alloy with molybdenum-coating, three piston rings

	Connecting rods
	Steel forged, trapezoid shaped small end, split big end

	Engine management
	Ford 2nd generation common rail diesel
engine management system

	Fuel injection
	Delphi common rail multiple injection
- tubular high-pressure common-rail with fuel pressure 2000 bar,
- 2 control valves (PCV/VCV), 3 pistons + internal transfer pump
- centrally located injectors, solenoid actuated, with 8-hole micro sac:
- closed loop 'minimum injection quantity' control


	Emission controls
	Oxidation catalyst, Water cooled EGR, Standard cDPF

	Emission level
	Euro Stage 5

	
	


Driveline
	Drive Options:
	AWD: All wheel drive 'Intelligent AWD-System' with variable torque distribution, electronically controlled, torque distribution up to 50:50; with electronic Haldex system.

	
	FWD: front wheel drive

	

	Transmissions:
	Ford Durashift 6-speed (MMT6 - Modular Manual Transmission 6-Speed): manual, fully synchronised transmission with shift cable and dual driveshaft

	(Option)
	Ford PowerShift (MPS6), electronically controlled 6-speed double-clutch transmission with dual driveshaft and wet clutches

	

	Ratios:

	
	2.0 Duratorq TDCi

140PS FWD/AWD and

163PS AWD

Durashift 6-sp manual
	2.0 Duratorq TDCi

140PS AWD and
163PS AWD

PowerShift 6-sp auto

	
	1. Gear
	3.583
	3.583

	
	2. Gear
	1.952
	1.952

	
	3. Gear
	1.241
	1.194

	
	4. Gear
	0.868
	0.842

	
	5. Gear
	0.943
	0.943

	
	6. Gear
	0.789
	0.789

	
	Reverse gear
	3.64
	4.843

	
	Final drive, 1 – 4

5, 6, R 
	4.533

3.238
	4.533

3.238


Weights
	
	
	
	
	Gross vehicle mass
	Axle loads

	
	Power
	Basic kerb1
	Payload
	
	front
	rear

	
	PS
	kg

	2.0 Duratorq TDCi, FWD 6-sp manual
	140
	1584
	476
	2060
	1120
	1080

	2.0 Duratorq TDCi, AWD 6-sp manual
	140/163
	1614
	516
	2130
	1140
	1115

	2.0 Duratorq TDCi, AWD 6-sp PowerShift
	140/163
	1672
	488
	2160
	1160
	1115


1 EG-basic kerb weight incl. driver (75 kg), lubricants and filled fuel tank (90%). All weights are valid for vehicles with basic specification.
	
	Towing limit / kg
	
	

	
	Trailer braked 12%
	Trailer unbraked
	Nose weight limit
	Roof weight limit

	2.0 Duratorq TDCi, 

FWD 6-sp manual
	2000
	750
	100
	75

	2.0 Duratorq TDCi,

AWD 6-sp manual
	2100
	750
	105
	75

	2.0 Duratorq TDCi,

AWD 6-sp PowerShift
	2100
	750
	105
	75


Off-Road Capabilities

	
	2.0 Duratorq TDCi, FWD
	2.0 Duratorq TDCi, AWD

	Max gradeability
	22°
	33°

	Max approach angle 
	14.5° with max axle load
	14.5° with max axle load

	Slope angle
	
	

	 front/rear

(with 4 persons, 68kg each, and 60kg luggage)
	21°/25°
	21°/25°

	Fording depth max.
	450 mm
	450 mm

	Ground clearance empty/laden to max rear axle load
	188/157 mm
	188/157 mm


Opomba: Navedeni podatki so bili v času priprave sporočila pravilni. Fordovo načelo nenehnega razvijanja produktov lahko pripelje do razlikovanja dejanskih podatkov. Pridržujemo si pravico do spremembe podatkov brez predhodnega opozorila.

# # #
Fordova obvestila o novostih in fotografije visoke ločljivosti so na voljo

na spletni strani podjetja Ford Motor Company za medije (http://media.ford.com).

 

Kontakt:

Katja Hvala

Odnosi z javnostmi

Summit motors Ljubljana

T 01 25 25 116

katja.hvala@summitmotors.si

Internet: http://media.ford.com

