Monster Fiesta Rally America Car 
Technical Data:

2.0-liter I-4 engine, mounted longitudinally, with Garrett turbocharger

Horsepower: Capable of 493 hp @ 8,000 rpm but Rally America required turbo-inlet restrictor will limit the engine to 330 hp @ 7,000 rpm

Torque: 553 lb.-ft. @ 6,000 rpm 

Maktrak/Olsbergs MSE 6-speed sequential transmission

Driveline: 4wd with front, center and rear mechanical differentials

15-inch Speedline magnesium wheels with Pirelli gravel-spec tires

Front suspension: modified MacPherson strut 

Rear suspension: double wishbones

Alcon 4-wheel disc brakes with 4-piston front and rear calipers

Steering: rack and pinion, 1.5 turns lock-to-lock

Body design by Olsbergs MSE: stock steel roof and doors; other panels are Kevlar and carbon fiber

Integrated rear wing and front spoiler

Vehicle weight: 2,900 lb. 

Acceleration: 0 to 62 mph in 3.5 seconds

Top speed: 155 mph

[image: image1.jpg]



