{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Latest"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Latest","index":0,"n_rows":100,"n_cols":9,"rows_kept":100,"merged":[[1,1,2,3],[1,4,2,5],[1,6,2,6],[1,7,2,8],[9,4,9,5],[9,7,9,8],[10,4,10,5],[10,7,10,8],[11,4,11,5],[11,7,11,8],[12,4,12,5],[12,7,12,8],[13,4,13,5],[13,7,13,8],[14,4,14,5],[14,7,14,8],[15,4,15,5],[15,7,15,8],[16,4,16,5],[16,7,16,8],[17,4,17,5],[17,7,17,8],[18,4,18,5],[18,7,18,8],[19,4,19,5],[19,7,19,8],[20,4,20,5],[20,7,20,8],[21,4,21,5],[21,7,21,8],[22,4,22,5],[22,7,22,8],[27,5,32,5],[27,8,32,8],[39,2,40,2],[39,4,39,8],[40,4,40,7],[41,4,41,8],[42,4,42,8],[43,2,44,2],[43,4,43,8],[44,4,44,8],[45,4,45,5],[45,7,45,8],[46,4,46,5],[46,7,46,8],[47,4,47,8],[48,4,48,6],[48,7,48,8],[49,4,49,6],[49,7,49,8],[50,4,50,7],[97,1,97,8],[98,1,98,8]],"flags":["formulas_cached_only"]}
[]
[null,"NISSAN JUKE tehnični podatki",null,null,"1.6-litrski bencinski motor",null,"1.5-litrski dizelski motor","1.6-litrski bencinski motor DIG-T"]
[]
[null,null,"Datum izdaje: Oktober 2010"]
[null,"MODEL"]
[null,null,"Nivoji opreme",null,"Visia, Acenta, Tekna","Acenta, Tekna","Visia, Acenta, Tekna","Acenta, Tekna","Acenta, Tekna"]
[null,null,"Število sedežev","oseb",5,5,5,5,5]
[]
[null,"POGONSKI SKLOP"]
[null,null,"Koda motorja",null,"HR16DE",null,"K9K","MR16DDT"]
[null,null,"Število valjev, razpored",null,"4, v vrsti",null,"4, v vrsti","4, v vrsti"]
[null,null,"Število ventilov na valj",null,4,null,2,4]
[null,null,"Air intake system",null,"Normal aspiration",null,"Turbocharger + Intercooler","Turbocharger + Intercooler"]
[null,null,"Prostornina motorja","cm³",1598,null,1461,1618]
[null,null,"Premer x hod","mm","Ø78 x 83.6",null,"Ø76 x 80.5","φ79.7 x 81.1"]
[null,null,"Največja moč motorja (1)","kW(KM)/min-1","86 (117) @ 6000",null,"81 (110) @ 4000","140 (190) @ 5600"]
[null,null,"Največji navor (1)","Nm/min-1","158Nm @ 4000",null,"240Nm @ 1750","240Nm @ 2000-5200"]
[null,null,"Kompresijsko razmerje",null,10.7,null,15.2,"9.5 : 1"]
[null,null,"Cam type",null,"DOHC led by chain",null,"SOHC led by belt","DOHC led by chain"]
[null,null,"Vrsta goriva",null,"Bencin",null,"Dizel","Bencin"]
[null,null,"Sistem vžiga",null,"individual coils / knock control",null,"Turbo polnilnik + Intercooler","Individual coils / Knock control"]
[null,null,"Dovod goriva",null,"Večtočkovni vbrizg goriva",null,"Common Rail Direktni Vbrizg","Sekvenčni High-pressure direktni vbrizg"]
[null,null,"Emisijska stopnja",null,"EU5",null,"EU5","EU5"]
[]
[null,"POGONSKI SKLOP"]
[null,null,"Vrsta sklopke",null,"dry single","Torque converter with lock-up","dry single","dry single","Torque converter with lock-up"]
[null,null,"Menjalnik",null,"5-stopenjski ročni","XTRONIC CVT","6-stopenjski ročni","6-stopenjski ročni","XTRONIC CVT-M6"]
[null,null,"Prestavna razmerja                 1.",null,3.727,"Low:4.006～HI:0.55",3.727,3.364,"Low:2.349～HI:0.394"]
[null,null,"2.",null,2.048,null,1.947,1.947]
[null,null,"3.",null,1.393,null,1.323,1.393]
[null,null,"4.",null,1.097,null,0.975,1.114]
[null,null,"5.",null,0.892,null,0.763,0.914]
[null,null,"6.",null,"-",null,0.638,0.767]
[null,null,"Vzvratna",null,3.545,3.771,3.687,3.292,1.751]
[null,null,"Transfer ratio",null,"-","－","-","-"]
[null,null,"Končno prestavno razmerje (Spredaj/Zadaj)",null,{"v":4.5,"d":"4.500"},3.754,4.214,4.214,5.798]
[null,null,"Pogon",null,"Sprednji","Sprednji","Sprednji","Sprednji","ALL-MODE 4x4-i w/Torque Vectoring"]
[]
[null,"ŠASIJA"]
[null,null,"Vzmetenje","spredaj","Posamična McPhersonova vzmetna noga, coil springs"]
[{"$nulls":3},"zadaj","Torsion beam axle, coil springs ",{"$nulls":3},"Multilink rear suspension"]
[null,null,"Upravljanje",null,"Električni servo ojačevalnik, zobata letev"]
[null,null,"Min. obračalni krog (med robnikoma)","m",10.7]
[null,null,"Zavorni sistem",null,"Diski spredaj, diski zadaj, diagonalni razdelilnik, servo ojačevalnik"]
[{"$nulls":4},"z ABS, EBD in sistemom za pomoč pri zaviranju v sili "]
[null,null,"Premer in debelina prednjih zavor","Φ","φ280 x 24",null,"φ280 x 24","φ296 x 26"]
[null,null,"Premer in debelina zadnjih zavor","Φ","φ292 x 9",null,"φ292 x 9","φ292 x 9"]
[null,null," ESP (Stability control system)",null,"standard"]
[null,null,"Velikost koles (glede na nivo opreme)",null,"16\"x 6.5\" (jeklo & alu) & 17\"x 7\" (alu)",null,null,"17\" x 7\" (alu)"]
[null,null,"Pnevmatike (glede na nivo opreme)",null,"VISIA, ACENTA : 205/60 R16 standardno (215/55R17 opcijsko)\nTEKNA : 215/55 R17 standardno",null,null,"215/55 R17"]
[null,null,"Velikost rezervne pnevmatike",null,"135/90 R16 (opcijsko)",{"$nulls":3},"135/90 R16 (standard)"]
[]
[null,"MASE IN MERE"]
[null,null,"Lastna teža min./max. (AT) (2)","kg","1172/1225","1213/1254","1285/1329","1286/1315","1425/1441"]
[null,null,"Skupna teža s tovorom (AT)","kg",1645,1675,1750,1735,1860]
[null,null,"Največja obremenitev (AT) (2)","kg",473,462,465,449,435]
[null,null,"Največja osna obremenitev (PAW)    spredaj","kg",870,895,965,960,1010]
[null,null,"                                      zadaj","kg",830,825,835,830,900]
[null,null,"Max. obrem. prikolice z zavoro","kg",1250,1250,1250,1200,1150]
[null,null,"                             brez zavore","kg",608,609,660,663,728]
[null,null,"Max. navpična obremenitev vlečne naprave","kg",75,75,75,75,75]
[null,null,"Max. obremenitev strehe","kg",75,75,75,75,75]
[null,null,"Celotna dolžina","mm",4135,4135,4135,4135,4135]
[null,null,"Celotna širina","mm",1765,1765,1765,1765,1765]
[null,null,"Celotna višina 2)","mm",1565,1565,1565,1565,1565]
[null,null,"Medosna razdalja","mm",2530,2530,2530,2530,2530]
[null,null,"Kolotek spredaj (16\" / 17\")","mm","1540 / 1525","1540 / 1525","1540 / 1525",1525,1525]
[null,null,"Kolotek zadaj (16\" / 17\")","mm","1535 / 1525","1535 / 1525","1535 / 1525",1525,1505]
[null,null,"Previs spredaj","mm",855,855,855,855,855]
[null,null,"Previs zadaj","mm",750,750,750,750,750]
[null,null,"Prtljažni prostor    - max. dolžina","mm","675 / 1470","675 / 1470","675 / 1470","675 / 1470","675 / 1470"]
[null,null,"                         - max. širina","mm",1409,1409,1409,1409,1409]
[null,null,"                         - max. višina do prekrivala prtljage","mm",403,403,403,403,403]
[null,null,"                         - max. višina do stropa","mm",681,681,681,681,681]
[null,null,"Prostornina prtljažnika (VDA)","l",251,251,251,251,207]
[null,null,"     max. z zloženimi sedeži (VDA) po bočni liniji","l",550,550,550,550,506]
[null,null,"     max. z zloženimi sedeži (VDA) do strehe","l",830,830,830,830,786]
[null,null,"Cd",null,0.35,0.35,0.35,0.35,0.35]
[null,null,"Kapaciteta rez. za gorivo","l",46,46,46,46,50]
[]
[null,"ZMOGLJIVOST"]
[null,null,"Poraba goriva"]
[null,null,"                    mesto","l/100 km",8.1,8.3,6.1,9.1,10.2]
[null,null,"                    izven mesta","l/100 km",5.3,5.2,4.5,5.6,{"v":6,"d":"6.0"}]
[null,null,"                    kombinirano","l/100 km",6.3,6.3,5.1,6.9,7.6]
[null,null,"Emisija CO2 (kombinirano)","g/km",147,145,134,159,175]
[null,null,"Pospešek 0 - 100 km/h","sek",{"v":11,"d":"11.0"},11.5,11.2,{"v":8,"d":"8.0"},8.4]
[null,null,"Največja hitrost","km/h",178,170,175,215,200]
[null,null,"Najmanjši obračalni krog","m",10.7,10.7,10.7,10.7,10.7]
[]
[null,"OFF-ROAD ZMOGLJIVOSTI"]
[null,null,"Kot približevanja","stopinj",26,26,26,26,26]
[null,null,"Kot oddaljevanja","stopinj",31,31,31,30,30]
[null,null,"Nagib","stopinj",22.5,22.5,22.5,22.5,23]
[null,null,"Minimalna višina od tal","mm",180,180,180,180,170]
[]
[null,"1) skladno s tehničnim predpisom 1999/99/EC."]
[null,"2) Vrednosti v skladu z direktivo ES. Masa praznega vozila pomeni maso brez voznika, a s hladilno tekočino, olji, gorivom, rezervno pnevmatiko in orodjem. Dovoljena obremenitev se zmanjša glede na opcije in/ali vgrajeno dodatno opremo. "]
[null,"3) V skladu z 93/116/ES. (Opcijska oprema, vzdrževanje, tehnika vožnje, cesta in vremenske razmere lahko vplivajo na uradne rezultate). "]
[null,"Opomba: Proizvajalec si pridržuje pravico do sprememb brez predhodnega obvestila."]