{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["FR","EN","ES","DE"],"not_rendered":{"images":4,"external_links":1,"defined_names":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"FR","index":0,"n_rows":26,"n_cols":3,"rows_kept":26,"flags":["formulas_cached_only"]}
[null,null,"TEHNIČNI PODATKI - Partner na električni pogon\nV fazi pridobitve homologacije "]
[null,null,"Povzetek - 09/2012"]
[]
["SPLOŠNI PODATKI","Tip","Električni pogon"]
[null,"Največja moč v kW (ali KM)","49 (67)"]
[null,"Največji navor (Nm)",200]
[null,"Pogonski akumulator: tip / zmogljivost (kW/h)","Litij-ionski / 22,5"]
[null,"Avtonomija po ciklu NEDC  (km)",170]
[]
["PORABA","Izpusti CO2 (g/km)",0]
[]
["DIMENZIJE (m)","Skupna dolžina vozila","D1: 4380 / D2: 4630 "]
[null,"Širina karoserije v predelu kljuk / pri zunanjih ogledalih v preklopljenem/razprtem položaju","1,810/ 1,857 / 2,112"]
[null,"Višina vozila pripravljenega za vožnjo (s polnimi rezervoarji)","1,801"]
[null,"Medosna razdalja","2,728"]
[null,"Previs SPR / Previs ZAD","0,925 / 0,727"]
[null,"Kolotek SPR / Kolotek ZAD","1,505 / 1,554"]
[]
["PROSTORNINA","Največja masa tovora (kg)","675"]
[null,"Prostornina prtljažnika (m3)","D1: 3,3 / 3,7(1) - D2: 3,7 / 4,1(1)"]
[]
[]
[]
[]
[]
[null,"(1) S sedežno klopjo MultiFlex "]

{"sheet":"EN","index":1,"n_rows":22,"n_cols":3,"rows_kept":22,"flags":["formulas_cached_only"]}
[null,null,"TECHNICAL CHARACTERISTICS - Partner Electric\nsous réserve d'homologation"]
[null,null,"Summary- 09/2012"]
[]
["GENERAL","Type","Electric"]
[null,"Max. power in kW (or bhp) / engine speed (rpm) ","49 (67)"]
[null,"Max. torque (Nm)/engine speed (rpm) ",200]
[null,"Traction battery type / capacity (kW.h)","Lithium-ion / 22,5"]
[null,"Autonomy NEDC cycle (km)",170]
[]
["FUEL CONSUMPTION","CO2 emissions (g/km) ",0]
[]
["DIMENSIONS (m)","Overall length","L1 : 4380 / L2 : 4630 "]
[null,"Body width including door handles / with door mirrors folded / open","1,810/ 1,857 / 2,112"]
[null,"Ride height","1,801"]
[null,"Wheelbase","2,728"]
[null,"Front overhang / Rear overhang ","0,925 / 0,727"]
[null,"Front track / Rear track","1,505 / 1,554"]
[]
["VOLUME","Total payload (kg)","675"]
[null,"Total load volume (m3)","L1 : 3,3 / 3,7(1) - L2 : 3,7 / 4,1(1)"]
[]
[null,"(1) With MultiFlex bench seat"]

{"sheet":"ES","index":2,"n_rows":22,"n_cols":3,"rows_kept":22,"flags":["formulas_cached_only"]}
[null,null,"CARACTERÍSTICAS TÉCNICAS - Parnter Electrique\nsous réserve d'homologation"]
[null,null,"Síntesis - 09/2012"]
[]
["GENERALIDADES","Type","Electrique"]
[null,"Potencia máxima en kW (o CV) / régimen (rpm) ","49 (67)"]
[null,"Par máximo (Nm) /  régimen (rpm) ",200]
[null,"Batterie de traction type / capacité (kW.h)","Lithium-ion / 22,5"]
[null,"Autonomie cycle NEDC  (km)",170]
[]
["CONSUMOS","Emisiones de CO2 (g/km)",0]
[]
["DIMENSIONES (m)","Longitud total","L1 : 4380 / L2 : 4630 "]
[null,"Anchura total / con retrovisores plegados / desplegados","1,810/ 1,857 / 2,112"]
[null,"Altura","1,801"]
[null,"Distancia entre ejes","2,728"]
[null,"Voladizo delantero / trasero","0,925 / 0,727"]
[null,"Vía delantera / trasera","1,505 / 1,554"]
[]
["VOLUMEN","Carga útil (kg)","675"]
[null,"Volumen de carga total  (m3)","L1 : 3,3 / 3,7(1) - L2 : 3,7 / 4,1(1)"]
[]
[null,"(1) Con banqueta MultiFlex   "]

{"sheet":"DE","index":3,"n_rows":20,"n_cols":3,"rows_kept":20,"flags":["formulas_cached_only"]}
[null,null,"TECHNISCHE DATEN - Partner Electrique\nsous réserve d'homologation"]
[null,null,"Synthese - 09/2012"]
[]
["ALLGEMEINES","Type","Electrique"]
[null,"max. Leistung in kW (PS) / bei Drehzahl (1/min)","49 (67)"]
[null,"max. Drehmoment (Nm) / bei Drehzahl (1/min)",200]
[null,"Batterie de traction type / capacité (kW.h)","Lithium-ion / 22,5"]
[null,"Autonomie cycle NEDC  (km)",170]
[]
["VERBRAUCH","CO2 -Ausstoß (g/km)",0]
[]
["ABMESSUNGEN (m)","Gesamtlänge","L1 : 4380 / L2 : 4630 "]
[null,"Breite an den Zierleisten / Rückspiegel angeklappt / über alles","1,810/ 1,857 / 2,112"]
[null,"Höhe fahrbereit ","1,801"]
[null,"Radstand","2,728"]
[null,"Überhang vorn / hinten","0,925 / 0,727"]
[null,"Spurbreite vorn / hinten","1,505 / 1,554"]
[]
["VOLUME","Charge utile (kg)"]
[null,"Volume de charge (m3)","L1 : 3,3 / 3,7(1) - L2 : 3,7 / 4,1(1)"]