{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Cruze HB5"],"not_rendered":{"external_links":1,"defined_names":1,"comments":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Cruze HB5","index":0,"n_rows":95,"n_cols":37,"rows_kept":95,"merged":[[0,1,0,31],[91,2,91,7]],"flags":["formulas_cached_only"]}
[null,"Tehnični podatki petvratnega modela Cruze"]
[null,"● Modelsko leto: 2012"]
[null,"● Trg: Evropa"]
[null,"● Stanje: 29. 5. 2011"]
[]
[null,"Pogonski sklop","1,6 l, RM","1,6 l, SM","1,8 l, RM","1,8 l, SM","2,0 l Euro5\nDizel, RM","2,0 l Euro5\nDizel, SM",null,"1.6L MT","1.6L MT","1.6L MT","1.6L AT","1.6L AT","1.6L AT","1.6L AT","1.6L AT","1.6L AT","1.8L MT","1.8L MT","1.8L AT","1.8L AT","1.8L AT -> MT","1.8L AT","1.8L AT","1.8L AT","2.0L Diesel MT","2.0L Diesel MT","2.0L Diesel MT","2.0L Diesel AT","2.0L Diesel AT","2.0L Diesel AT",null,"1.8L MT","1.8L AT","2.0L Diesel MT","2.0L Diesel AT"]
[null,"Podatki o motorju"]
[null,"Motor, položaj","spredaj, prečno\npred osjo","spredaj, prečno\npred osjo","spredaj, prečno\npred osjo","spredaj, prečno\npred osjo","spredaj, prečno\npred osjo","spredaj, prečno\npred osjo",null,"front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle",null,"front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle","front, transverse in front of axle"]
[null,"Hladilni sistem","s tekočino, zaprt krogotok","s tekočino, zaprt krogotok","s tekočino, zaprt krogotok","s tekočino, zaprt krogotok","s tekočino, zaprt krogotok","s tekočino, zaprt krogotok",null,"with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit",null,"with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit","with liquid, sealed circuit"]
[null,"Število valjev",4,4,4,4,4,4,null,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,null,4,4,4,4]
[null,"Izvrtina (mm)",79,79,80.5,80.5,"86","86",null,79,79,79,79,79,79,79,79,79,80.5,80.5,80.5,80.5,80.5,80.5,80.5,80.5,"83.0","83.0","83.0","83.0","83.0","83.0",null,80.5,80.5,"83.0","83.0"]
[null,"Hod (mm)",81.5,81.5,88.2,88.2,"86","86",null,81.5,81.5,81.5,81.5,81.5,81.5,81.5,81.5,81.5,88.2,88.2,88.2,88.2,88.2,88.2,88.2,88.2,"92.0","92.0","92.0","92.0","92.0","92.0",null,88.2,88.2,"92.0","92.0"]
[null,"Gibna prostornina (cm3)",1598,1598,1796,1796,1998,1998,null,1598,1598,1598,1598,1598,1598,1598,1598,1598,1796,1796,1796,1796,1796,1796,1796,1796,1991,1991,1991,1991,1991,1991,null,1796,1796,1991,1991]
[null,"Razmerje kompresije","11.0 : 1","11.0 : 1","10.5 : 1","10.5 : 1","16.5 : 1","16.5 : 1",null,"9.5:1","9.5:1","9.5:1","9.5:1","9.5:1","9.5:1","9.5:1","9.5:1","11.0 : 1","10.5 : 1","10.5 : 1","10.5 : 1","10.5 : 1","10.5 : 1","10.5 : 1","10.5 : 1","10.5 : 1","17.5 : 1","17.5 : 1","17.5 : 1","17.5 : 1","17.5 : 1","17.5 : 1",null,"10.5 : 1","10.5 : 1","17.5 : 1","17.5 : 1"]
[null,"Vrsta motorja","vrstni; 4","vrstni; 4","vrstni; 4","vrstni; 4","vrstni; 4 ","vrstni; 4 ",null,"in line 4","in line 4","in line 4","in line 4","in line 4","in line 4","in line 4","in line 4","in line; 5 main bearings","in line; 5 main bearings","in line; 5 main bearings","in line; 5 main bearings","in line; 5 main bearings","in line; 5 main bearings","in line; 5 main bearings","in line; 5 main bearings","in line; 5 main bearings","in line 4","in line 4","in line 4","in line 4","in line 4","in line 4",null,"in line; 5 main bearings","in line; 5 main bearings","in line 4","in line 4"]
[null,"Odmične gredi, mesto","DOHC,\ngnani z zobatim jermenom","DOHC,\ngnani z zobatim jermenom","DOHC,\ngnani z zobatim jermenom","DOHC,\ngnani z zobatim jermenom","DOHC,\ngnani z verigo","DOHC,\ngnani z verigo",null,"2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","1 overhead (SOHC), driven by toothed belt","1 overhead (SOHC), driven by toothed belt","1 overhead (SOHC), driven by toothed belt","1 overhead (SOHC), driven by toothed belt","1 overhead (SOHC), driven by toothed belt","1 overhead (SOHC), driven by toothed belt",null,"2 overhead (DOHC), driven by toothed belt","2 overhead (DOHC), driven by toothed belt","1 overhead (SOHC), driven by toothed belt","1 overhead (SOHC), driven by toothed belt"]
[null,"Ventilni sklop","DOHC, 16-ventilni","DOHC, 16-ventilni","DOHC, 16-ventilni","DOHC, 16-ventilni","DOHC, 16-ventilni","DOHC, 16-ventilni",null,"DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","DOHC 16 valve","SOHC 16 valve","SOHC 16 valve","SOHC 16 valve","SOHC 16 valve","SOHC 16 valve","SOHC 16 valve",null,"DOHC 16 valve","DOHC 16 valve","SOHC 16 valve","SOHC 16 valve"]
[null,"Razporeditev ventilov","v; 4 na valj","v; 4 na valj","v; 4 na valj","v; 4 na valj","4 na valj","4 na valj",null,"v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","v; 4 per cylinder","4 per cylinder","4 per cylinder","4 per cylinder","4 per cylinder","4 per cylinder","4 per cylinder",null,"v; 4 per cylinder","v; 4 per cylinder","4 per cylinder","4 per cylinder"]
[null,"Prilagajanje ventilov","mehanski dročnik","mehanski dročnik","mehanski dročnik","mehanski dročnik","samodejno hidravlično","samodejno hidravlično",null,"automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","mechanical tappet","mechanical tappet","mechanical tappet","mechanical tappet","mechanical tappet","mechanical tappet","mechanical tappet","mechanical tappet","mechanical tappet","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic","automatic-hydraulic",null,"mechanical tappet","mechanical tappet","automatic-hydraulic","automatic-hydraulic"]
[null,"Dovod goriva","večtočkovno vbrizgavanje","večtočkovno vbrizgavanje","večtočkovno vbrizgavanje","večtočkovno vbrizgavanje","vbrizgavanje s skupnim vodom","vbrizgavanje s skupnim vodom",null,"Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","Multi-Point Injection","common rail injection","common rail injection","common rail injection","common rail injection","common rail injection","common rail injection",null,"Multi-Point Injection","Multi-Point Injection","common rail injection","common rail injection"]
[null,"Sistem vžiga","sistem neposrednega vžiga","sistem neposrednega vžiga","sistem neposrednega vžiga","sistem neposrednega vžiga","-","-",null,"DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","DIS","-","-","-","-","-","-",null,"DIS","DIS","-","-"]
[null,"Črpalka za gorivo","elektromotor","elektromotor","elektromotor","elektromotor","elektromotor","elektromotor",null,"Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","Electric Motor","electric motor","electric motor","electric motor","electric motor","electric motor","electric motor",null,"Electric Motor","Electric Motor","electric motor","electric motor"]
[null,"Sistem upravljanja izpustov","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","DELPHI EMS","DELPHI EMS",null,"DELPHI EMS","DELPHI EMS","DELPHI EMS","DELPHI EMS","DELPHI EMS","DELPHI EMS","DELPHI EMS","DELPHI EMS","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","Siemens SIM2K-76","Bosch EMS ","Bosch EMS ","Bosch EMS ","Bosch EMS ","Bosch EMS ","Bosch EMS ",null,"Siemens SIM2K-76","Siemens SIM2K-76","Bosch EMS ","Bosch EMS "]
[null,"Moč (kW/KM pri 1/min)","(91.2 / 124 @ 6400)","(91.2 / 124 @ 6400)","(104 / 141 @ 6200)","(104 / 141 @ 6200)","120/163 @ 3800","120/163 @ 3800",null,"80/109 @ 6000","80/109 @ 6000","80/109 @ 6000","80/109 @ 6000","80/109 @ 6000","80/109 @ 6000","80/109 @ 6000","80/109 @ 6000","(88.4 / 120.2@6400)","(104 / 141@6200)","(104 / 141@6200)","(104 / 141@6200)","(104 / 141@6200)","(104 / 141@6200)","(104 / 141@6200)","(104 / 141@6200)","(104 / 141@6200)","110/150 @ 4000","110/150 @ 4000","110/150 @ 4000","110/150 @ 4000","110/150 @ 4000","110/150 @ 4000",null,"(104 / 141@6200)","(104 / 141@6200)","110/150 @ 4000","110/150 @ 4000"]
[null,"Specifična moč (kW/l; KM/l)","56.0 ; 76.2","56.0 ; 76.2","57.8 ; 78.3","57.8 ; 78.3","60.1 ; 81.6","60.1 ; 81.6",null,"50 / 68.2","50 / 68.2","50 / 68.2","50 /68.2","50 /68.2","50 /68.2","50 /68.2","50 /68.2","55.3 ; 75.2","57.8 ; 78.3","57.8 ; 78.3","57.8 ; 78.3","57.8 ; 78.3","57.8 ; 78.3","57.8 ; 78.3","57.8 ; 78.3","57.8 ; 78.3","55.2; 75.3","55.2; 75.3","55.2; 75.3","55.2; 75.3","55.2; 75.3","55.2; 75.3",null,"57.8 ; 78.3","57.8 ; 78.3","55.2; 75.3","55.2; 75.3"]
[null,"Največji navor (Nm pri 1/min)","(154 @ 4200)","(154 @ 4200)","(176 @ 3800)","(176 @3800)","360 @ 1750~2750","360 @ 1750~2750",null,"150 @ 4000","150 @ 4000","150 @ 4000","150 @ 4000","150 @ 4000","150 @ 4000","150 @ 4000","150 @ 4000","(149.1 @4200)","(176 @3800)","(176 @3800)","(176 @3800)","(176 @3800)","(176 @3800)","(176 @3800)","(176 @3800)","(176 @3800)","320 @ 2000","320 @ 2000","320 @ 2000","320 @ 2000","320 @ 2000","320 @ 2000",null,"(176 @3800)","(176 @3800)","320 @ 2000","320 @ 2000"]
[null,"Specifični navor (Nm/l)",95.2,95.2,{"v":97.77777777777777,"d":"97.8"},"97.8","180.2","180.2",null,93.8,93.8,93.8,93.8,93.8,93.8,93.8,93.8,{"v":93,"d":"93.0"},{"v":97.77777777777777,"d":"97.8"},{"v":97.77777777777777,"d":"97.8"},{"v":97.77777777777777,"d":"97.8"},{"v":97.77777777777777,"d":"97.8"},{"v":97.77777777777777,"d":"97.8"},{"v":97.77777777777777,"d":"97.8"},{"v":97.77777777777777,"d":"97.8"},{"v":97.77777777777777,"d":"97.8"},"155.7","155.7","155.7","155.7","155.7","155.7",null,{"v":97.77777777777777,"d":"97.8"},{"v":97.77777777777777,"d":"97.8"},"155.7","155.7"]
[null,"Povprečni dejanski tlak pri","1050,1 pri največji moči","1050,1 pri največji moči","1120,8 pri največji moči","1120,8 pri največji moči","22,64 bara","22,64 bara",null,1001.3,1001.3,1001.3,1001.3,1001.3,1001.3,1001.3,1001.3,"1037.2 @ max power","1120.8 @ max power","1120.8 @ max power","1120.8 @ max power","1120.8 @ max power","1120.8 @ max power","1120.8 @ max power","1120.8 @ max power","1120.8 @ max power",{"v":2020,"d":"2020.0"},{"v":2020,"d":"2020.0"},{"v":2020,"d":"2020.0"},{"v":2020,"d":"2020.0"},{"v":2020,"d":"2020.0"},{"v":2020,"d":"2020.0"},null,"1120.8 @ max power","1120.8 @ max power",{"v":2020,"d":"2020.0"},{"v":2020,"d":"2020.0"}]
[null,"pri največji moči/navoru (kPa)","1196,3 pri največjem navoru","1196,3 pri največjem navoru","1230,8 pri največjem navoru","1230,8 pri največjem navoru","1897 pri največji moči","1897 pri največji moči",null,"1179 @ max torque","1179 @ max torque","1179 @ max torque","1179 @ max torque","1179 @ max torque","1179 @ max torque","1179 @ max torque","1179 @ max torque","1171.9 @ max power","1230.8 @ max torque","1230.8 @ max torque","1230.8 @ max torque","1230.8 @ max torque","1230.8 @ max torque","1230.8 @ max torque","1230.8 @ max torque","1230.8 @ max torque","1657 @ max torque","1657 @ max torque","1657 @ max torque","1657 @ max torque","1657 @ max torque","1657 @ max torque",null,"1230.8 @ max torque","1230.8 @ max torque","1657 @ max torque","1657 @ max torque"]
[null,"Povprečna hitrost bata (m/s)",17.4,17.4,18.2,18.2,"13.8","13.8",null,"16.3","16.3","16.3","16.3","16.3","16.3","16.3","16.3",17.4,18.2,18.2,18.2,18.2,18.2,18.2,18.2,18.2,14.1,14.1,14.1,14.1,14.1,14.1,null,18.2,18.2,14.1,14.1]
[null,"Prostornina motornega olja (l)",4.5,4.5,4.5,4.5,"7.3","7.3",null,"3.75L","3.75L","3.75L","3.75L","3.75L","3.75L","3.75L","3.75L","4.5L","4.5L","4.5L","4.5L","4.5L","4.5L","4.5L","4.5L","4.5L","6.5L","6.5L","6.5L","6.5L","6.5L","6.5L",null,"4.5L","4.5L","6.5L","6.5L"]
[null,"Prostornina hladilne tekočine (l)",6.3,6.3,6.3,6.3,"10.0","      10.010",null,"6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","6.3L","10L","10L","10L","10L","10L","10L",null,"6.3L","6.3L","10L","10L"]
[null,"Akumulator 12 V, zmogljivost (Ah)","60 A","60 A","60 A","60 A","75 A","75 A",null,"60A","60A","60A","60A","60A","60A","60A","60A","60A","60A","60A","60A","60A","60A","60A","60A","60A","75A","75A","75A","75A","75A","75A",null,"60A","60A","75A","75A"]
[null,"Alternator 14,2 V, zmogljivost (W)","100 A","100 A","100 A","100 A","140 A","140 A",null,"100A","100A","100A","100A","100A","100A","100A","100A","100A","100A","100A","100A","100A","100A","100A","100A","100A","140A","140A","140A","140A","140A","140A",null,"100A","100A","140A","140A"]
[null,"Menjalnik"]
[null,"Pogonska os","pogon na sprednjih kolesih","pogon na sprednjih kolesih","pogon na sprednjih kolesih","pogon na sprednjih kolesih","pogon na sprednjih kolesih","pogon na sprednjih kolesih",null,"front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive","front wheel drive",null,"front wheel drive","front wheel drive","front wheel drive","front wheel drive"]
[null,"Vrsta menjalnika","ročni","samodejni","ročni","samodejni","ročni","samodejni",null,"Manual","Manual","Manual","Automatic","Automatic","Automatic","Automatic","Automatic","Automatic","Manual","Manual","Automatic","Automatic","Automatic","Automatic","Automatic","Automatic","Manual","Manual","Manual","Automatic","Automatic","Automatic",null,"Manual","Automatic","Manual","Automatic"]
[null,"Prestavna razmerja","3.81/2.158/1.481/1.121/\n0,886/vzv. 3.545/RKP: 3.944","4.449/2.908/1.893/1.446/0,742/vzv. 2,871/RKP 4,11","3.818/2.158/1.481/1.121/\n0,886/vzv. 3.545/RKP: 3.722","4.449/2.908/1.893/1.446/0,742/vzv. 2,871/\nRKP: 3.72","4.167/2.130/1.321/0.954/\n0.755/0.623/\nvzv. 3.917/RKP:3.348","4.584/2.964/1.912/1.446/0,746/vzv. 2,94/RKP: 2.64",null,"3.818/2,158/1.481/1.121/0.886/Rev3.545/FDR3.944","3.818/2,158/1.481/1.121/0.886/Rev3.545/FDR3.944","3.818/2,158/1.481/1.121/0.886/Rev3.545/FDR3.944","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR 3.87","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR 3.87","4.449/2.908/1.893/1.446/1/0.742/Rev 2.871/FDR 4.11","4.449/2.908/1.893/1.446/1/0.742/Rev 2.871/FDR 4.11","4.449/2.908/1.893/1.446/1/0.742/Rev 2.871/FDR 4.11","4.449/2.908/1.893/1.446/1/0.742/Rev 2.871/FDR 4.11","3.818/2,158/1.481/1.121/0.886/Rev3.545/FDR3.722","3.818/2,158/1.481/1.121/0.886/Rev3.545/FDR3.722","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR:3.23 or 3.87","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR 3.23 or 3.87",null,"4.449/2.908/1.893/1.446/1/0.742/Rev 2.871/FDR 3.72","4.449/2.908/1.893/1.446/1/0.742/Rev 2.871/FDR 3.72","4.449/2.908/1.893/1.446/1/0.742/Rev 2.871/FDR 3.72","3.947/2.036/1.348/0.971/0.721/Rev:3.615/FDR:3.261","3.947/2.036/1.348/0.971/0.721/Rev:3.615/FDR:3.261","3.947/2.036/1.348/0.971/0.721/Rev:3.615/FDR:3.261","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR 2.29","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR 2.30","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR 2.31",null,"3.818/2,158/1.481/1.121/0.886/Rev3.545/FDR3.944","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR3.23","3.947/2.194/1.348/0.971/0.721/Rev:3.615/FDR:3.421","4.584/2.964/1.912/1.446/1/0.746/Rev -2.94/FDR 2.29"]
[null,"Vrsta sklopke","suha, enojna","-","suha, enojna","-","suha, enojna","-",null,"dry, single disc","dry, single disc","dry, single disc","-","-","-","-","-","-","dry, single disc","dry, single disc","-","-","-","-","-","-","dry, single disc","dry, single disc","dry, single disc","-","-","-",null,"dry, single disc","-","dry, single disc","-"]
[null,"Karoserija"]
[null,"Sedeži",5,5,5,5,5,5,null,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,5,null,5,5,5,5]
[null,"Koeficient upora (cd)",0.352,0.352,0.352,0.352,0.352,0.352,null,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,0.306,null,0.306,0.306,0.306,0.306]
[null,"Sprednji del (A v m2)",2.217,2.217,2.217,2.217,2.217,2.217,null,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,2.217,null,2.217,2.217,2.217,2.217]
[null,"Indeks (cw xA)",{"v":0.780384,"d":"0.780"},{"v":0.780384,"d":"0.780"},{"v":0.780384,"d":"0.780"},{"v":0.780384,"d":"0.780"},{"v":0.780384,"d":"0.780"},{"v":0.78,"d":"0.780"},null,{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},null,{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"},{"v":0.6784020000000001,"d":"0.678"}]
[null,"Podvozje"]
[null,"Vzmetenje sprednjih koles","vzmetna noga McPherson","vzmetna noga McPherson","vzmetna noga McPherson","vzmetna noga McPherson","vzmetna noga McPherson","vzmetna noga McPherson",null,"McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut",null,"McPherson Strut","McPherson Strut","McPherson Strut","McPherson Strut"]
[null,"Vzmetenje zadnjih koles","sestavljena ročična gred","sestavljena ročična gred","sestavljena ročična gred","sestavljena ročična gred","sestavljena ročična gred","sestavljena ročična gred",null,"Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle",null,"Compound Crank Axle","Compound Crank Axle","Compound Crank Axle","Compound Crank Axle"]
[null,"Zavore"]
[null,"Zavorni krogotok","X-diagonale","X-diagonale","X-diagonale","X-diagonale","X-diagonale","X-diagonale",null,"X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals","X-diagonals",null,"X-diagonals","X-diagonals","X-diagonals","X-diagonals"]
[null,"Premer sprednjih zavor (mm)","hlajene kolutne zavore, 276","hlajene kolutne zavore, 276","hlajene kolutne zavore, 276","hlajene kolutne zavore, 276","hlajene kolutne zavore, 300","hlajene kolutne zavore, 300",null,"15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","15\" Vent Disk","16\" Vent Disk","16\" Vent Disk","16\" Vent Disk","16\" Vent Disk","16\" Vent Disk","16\" Vent Disk",null,"15\" Vent Disk","15\" Vent Disk","16\" Vent Disk","16\" Vent Disk"]
[null,"Premer zadnjih zavor (mm)","kolutne zavore s trdim sedlom, 268","kolutne zavore s trdim sedlom, 268","kolutne zavore s trdim sedlom, 268","kolutne zavore s trdim sedlom, 268","kolutne zavore s trdim sedlom, 292","kolutne zavore s trdim sedlom, 292",null,"15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","16\" Solid Disk","16\" Solid Disk","16\" Solid Disk","16\" Solid Disk","16\" Solid Disk","16\" Solid Disk",null,"15\" Solid Disk/15\" Drum Brake","15\" Solid Disk/15\" Drum Brake","16\" Solid Disk","16\" Solid Disk"]
[null,"ABS","4-kanalni, 4-tipalni","4-kanalni, 4-tipalni","4-kanalni, 4-tipalni","4-kanalni, 4-tipalni","4-kanalni, 4-tipalni","4-kanalni, 4-tipalni",null,"4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor",null,"4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor","4ch, 4 sensor"]
[null,"Teže in mere"]
[null,"Zunanje mere"]
[null,"Dolžina (mm)",4510,4510,4510,4510,4510,4510,null,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,4597,null,4597,4597,4597,4597]
[null,"Širina (mm)",1797,1797,1797,1797,1797,1797,null,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,1788,null,1788,1788,1788,1788]
[null,"Višina (mm)",1477,1477,1477,1477,1477,1477,null,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,1477,null,1477,1477,1477,1477]
[null,"Medosna razdalja (mm)",2685,2685,2685,2685,2685,2685,null,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,2685,null,2685,2685,2685,2685]
[null,"Kolotek spredaj/zadaj (mm)","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558",null,"1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558","1544/1558",null,"1544/1558","1544/1558","1544/1558","1544/1558"]
[null,"Notranje mere"]
[null,"Prostor za noge spredaj/zadaj (mm) ","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917",null,"1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917","1074/917",null,"1074/917","1074/917","1074/917","1074/917"]
[null,"Prostor za rame spredaj/zadaj (mm) ","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370",null,"1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370","1391/1370",null,"1391/1370","1391/1370","1391/1370","1391/1370"]
[null,"Prostor za glavo spredaj/zadaj (mm) ","999/974","999/974","999/974","999/974","999/974","999/974",null,"999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963","999/963",null,"999/963","999/963","999/963","999/963"]
[null,"Prostornina prtljažnika (dvignjen/zložen sedež) (I)","413/883","413/883","413/883","413/813","413/883","413/883",null,"450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)","450(VDA)",null,"450(VDA)","450(VDA)","450(VDA)","450(VDA)"]
[]
[null,"Širina platišč (palci)(mm)/velikost pnevmatik","6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx16/205/60R16\n7Jx17/225/50R17","6.5Jx16/205/60R16\n7Jx17/225/50R17",null,"6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17",null,"6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17","6.5Jx15/205/65R15\n6.5Jx16/205/60R16\n7Jx17/215/50R17"]
[null,"Polmer kroga obračanja; najmanjši/med dvema zidovoma (m)","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4",null,"10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4",null,"10.9/11.4","10.9/11.4","10.9/11.4","10.9/11.4"]
[null,"Krmilni mehanizem","hidravlično servokrmiljenje","hidravlično servokrmiljenje","hidravlično servokrmiljenje","hidravlično servokrmiljenje","hidravlično servokrmiljenje","hidravlično servokrmiljenje",null,"hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering",null,"hydraulic power steering","hydraulic power steering","hydraulic power steering","hydraulic power steering"]
[null,"Zunanji premer krmila (mm)",370,370,370,370,370,370,null,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,370,null,370,370,370,370]
[null,"Skupna teža vozila/najv. dovoljena teža (GVW) (kg)","1305/1818","1315/1828","1310/1823","1319/1832","1480/1993","1510/2023"]
[null,"Razmerje moč/teža (kg/kW; kg/KM)(prazen)",14.3,14.5,12.6,12.6,12.3,12.6]
[null,"Največja osna obremenitev spredaj/zadaj (kg)","1060/1000","1060/1000","1060/1000","1060/1000","1140/1000","1140/1000"]
[null,"Teža prikolice – z zavorami (kg)",1200,1200,1200,1200,1200,1200]
[null,"Teža mehanske priklopne spojke (kg)",75,75,75,75,75,75,null,"75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg","75kg",null,"75kg","75kg","75kg","75kg"]
[null,"Teža sklopa kljuke (kg)",25,25,25,25,25,25,null,"25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg","25kg",null,"25kg","25kg","25kg","25kg"]
[null,"Prostornina posode za gorivo (l)",60,60,60,60,60,60,null,"60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l","60l",null,"60l","60l","60l","60l"]
[null,"Zmogljivost"]
[null,"Najvišja hitrost (km/h)",190,185,200,195,205,209,null,"≥ 180","≥ 180","NQR Mean ??",177,"NQR Mean ??","≥ 178","≥ 177","NQR Mean ??","≥ 180","≥ 195","←","≥ 190","←","≥ 195","≥ 190","≥ 190","←",208,"←","←",206,"←","←",null,197,190,206,"N/A"]
[null,"Pospešek 0–100 km/h (s)",{"v":12,"d":"12.0"},12.7,10.1,10.4,8.5,9.8,null,"≤ 13.1","≤ 13.5",null,13.5,null,"≤ 14.2","≤ 14.5",null,"≤ 13","≤ 11.0","←","≤ 12.0","←","≤ 10.5","≤ 11.5","≤ 12.0","←",9.3,"←","←",10.4,"←","←",null,10.1,11.5,8.8,"N/A"]
[null,"Posp. 40–100 km/h v 4. prestavi (s)",18.9,{"v":11,"d":"11.0"},17.3,9.1,13.1,8.5,null,"≤ 19","≤ 19",null,11.9,null,"≤ 12.7","≤ 13",null,"≤ 11","≤  18.5","←","≤  10.5","←","≤  17.0","≤ 10.0","≤ 10.5","←",16.1,"←","←",8.3,"←","←",null,15.9,{"v":10,"d":"10.0"},14.6,"N/A"]
[null,"Posp. 80–120 km/h v 5. prestavi (s)",{"v":20,"d":"20.0"},11.1,17.9,9.3,10.7,8.4,null,"≤ 20","≤ 20.5",null,12.9,null,"≤ 13.7","≤ 14",null,"≤ 11.5","≤ 19.0","←","≤ 10.5","←","≤ 16.0 /≤ 12.5 ","≤ 10.5","≤ 10.5","←",12.9,"←","←",9.9,"←","←",null,15.9,9.7,11.7,"N/A"]
[null,"Zunanji hrup pri vožnji (dBA)",71.8,71.6,72.5,73.4,71,69.2]
[null,"Gorivo","bencin (neosvinčen)","bencin (neosvinčen)","bencin (neosvinčen)","bencin (neosvinčen)","dizel","dizel",null,"Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Leaded)","Gasoline (Unleaded)","Gasoline (Leaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Leaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Gasoline (Unleaded)","Diesel","Diesel","Diesel","Diesel","Diesel","Diesel",null,"Gasoline","Gasoline","Diesel","Diesel"]
[null,"Poraba goriva (l/100 km)",6.6,7.4,6.6,7.4,5.6,6.3,null,"≤ 7.3","≤ 7.4",null,8.1,null,"≤ 8.3","≤ 8.4",null,"≥ 13","≤ 6.9","←","≤ 8.1","←","≤ 7.3","≤ 7.6","≤ 7.7","←",5.6,null,null,6.7,{"$nulls":3},7.1,7.6,5.7,"N/A"]
[null,"Poraba goriva pri mestni vožnji",8.9,10.3,8.9,10.7,7.7,8.7]
[null,"Poraba goriva pri vožnji zunaj mesta",5.2,5.7,5.2,5.5,4.4,5]
[null,"Emisije CO2 (g/km)",153,174,155,174,147,167,{"$nulls":15},179,183,"←",149,null,null,177,{"$nulls":3},169,181,155,"N/A"]
[null,"Emisije CO2 (g/km), mestna vožnja",208,242,210,252,202,229]
[null,"Emisije CO2 (g/km), zunaj mesta",122,133,123,130,115,131]
[null,"Emisijski razred","Euro5","Euro5","Euro5","Euro5","Euro5","Euro5",null,"Euro4","Euro3",null,"Euro3",null,"Euro4","Euro3",null,"KULEV","Euro4","Euro3","Euro4","Euro3","Euro3","Euro5","Euro4","Euro3","Euro4","Euro3","Euro2","Euro4","Euro3","Euro2",null,"Euro3","Euro3","Euro3","Euro3"]
[]
[{"$nulls":9},"FDR3.944","FDR3.944",null,"6T40, FDR3.87","6T40, FDR3.87","6T30,FDR4.11","6T30,FDR4.11",null,"6T30,FDR4.11","FDR3.722",null,"6T40,FDR3.87","6T40,FDR3.87","M32","6T30,FDR3.72","6T30,FDR3.72","6T30,FDR3.72",{"$nulls":7},"FDR3.944","6T40 FDR3.23","FDR:3.421, 2nd:2.194","None sale?"]
[{"$nulls":9},"RoN91","RoN87",null,"RoN95",null,"RoN91","RoN87",null,"RoN93","RoN91",null,"RoN91","RoN91","RoN91","RoN95","RoN91","RoN91",{"$nulls":7},"RoN95","RoN95"]
[{"$nulls":12},"Perf. : MY10 Euro4 status C/O",{"$nulls":8},"Andean?","Andean?","Perf. : MY11 Europe VTS C/O",null,null,"Perf. : MY10 Europe status C/O","←","←","Perf. : MY10 Europe status C/O","←","←",null,"Perf:  Simulaton","Perf: Euro status C/O","Perf: Simulaton"]
[{"$nulls":23},"FE: MY11 Europe VTS C/O","FE : diffence of each market","←","FE : MY10 Europe status C/O","FE : diffence of each market","←","FE : MY10 Europe status C/O","FE : diffence of each market","←",null,"FE : Certi.","FE : Certi.","FE : Certi."]