## **NEW NISSAN JUKE TECHNICAL DATA**

|  |  |
| --- | --- |
| **Engine** | Turbocharged 1.0 l (999 cc) three-cylinder gasolineE6D-TEMP |
| **Power and torque output** | 117 PS / 86 kW @ 5,250 RPM180 Nm @ 1,750 RPM200 Nm (with Over Torque function1) |
| **Transmission** | Six-speed manual (6MT) | Seven-speed dual clutch (DCT7) |
| **Acceleration (0-100 km/h) (secs)** | 10.4 |  11.1(provisional) |
| **Maximum speed (km/h)** | 180 | 180 |
| **Wheels/tyres** | * 16 inch steel - 215/65 (standard on Visia grade)
* 17 inch alloy – 215/60 (standard from Acenta)
* 19 inch alloy – 225/45 (optional on Tekna )
 |
| **Front suspension** | Macpherson Strut type |
| **Rear suspension** | Twist beam, coil spring type |
| **Brakes front/rear** | Disc, 280 mm / Disc, 260 mm (from N-Connecta)w/ ABS, BA, EBD, TCS, VDC |
| **Exterior dimensions (mm)** | * Length: 4,210
* Width: 1,800
* Height: 1,595
* Wheelbase: 2,636
 |
| **Rear cabin dimensions (mm)** | * Rear knee room: 583
* Rear head room: 22
* Rear shoulder room: 1,320.3
 |
| **Luggage space capacity and dimensions** | * Max. boot aperture width (mm): 1,072
* Base boot aperture width (mm): 1,003
* Luggage capacity (l): 422
 |
| **Min. kerb weight****(N-Connecta)(kg)** | 1,192(provisional) | 1,210(provisional) |
| **Infotainment and connectivity** | * NissanConnect in-car infotainment system with 8 inch touch screen display (standard on Acenta, N-Connecta, Tekna)
	+ Apple® CarPlay, Android® Auto\*
* NissanConnect Services (option on Acenta, N-Connecta, Tekna)
	+ Nissan on Google Assistant\*
	+ In-Car WiFI\*\*\*
	+ Driving History & Analysis\*
	+ Maps & Live Traffic\*\*
	+ Nissan Help & Support\*
	+ Breakdown Call\*
	+ Vehicle Health\*
	+ Smart Alerts\*\*
* Colour TFT screen (4.2 inch standard on Visia, Acenta, 7 inch standard on N-Connecta, Tekna)
* BOSE® Personal® Plus sound system (option from N-Connecta)
	+ Eight speakers, including UltraNearFIeld headrest speakers for driver and front passenger
 |
| **Safety features** | * Standard on all grades safety functionalities
	+ Emergency Call\*
	+ Cruise Control & Speed Limiter
	+ Intelligent Emergency Braking with Pedestrian & Cyclist Recognition
	+ Intelligent Lane Intervention and Warning
	+ High Beam Assist
	+ Traffic Sign Recognition linked to Cruise Control
	+ Hill Start Assist
* Intelligent Cruise Control (standard on Tekna; option on N-Connecta )
* Nissan ProPILOT (standard on Tekna; option on N-Connecta)
* Around View Monitor (standard on Tekna; option on N-Connecta)
* Intelligent Driver Alertness (standard on Tekna; option on N-Connecta)
* Blind Spot Intervention (standard on Tekna; option on N-Connecta)
* Rear Cross-Traffic Alert (standard on Tekna; option on N-Connecta)
 |
| **Seating capacity** | 5 |
| **Warranty** | 3 years / 100,000 km |

**\* Free for seven years, then pay per use. Availability depending on your country or region.**

**\*\* Free for three years, then pay per use. Availability depending on your country or region.**

**\*\*\* Paid only Availability depending on your country or region.**

**1 Over Torque function provides an additional 20 Nm for 25 seconds upon application of full throttle. The function is applied from second gear through to the longest gear.**

**2 19 inch standard application on Tekna according to country**