## **NEW NISSAN JUKE TECHNICAL DATA**

|  |  |  |  |
| --- | --- | --- | --- |
| **Engine** | Turbocharged 1.0 l (999 cc) three-cylinder gasoline  E6D-TEMP | | |
| **Power and torque output** | 117 PS / 86 kW @ 5,250 RPM  180 Nm @ 1,750 RPM  200 Nm (with Over Torque function1) | | |
| **Transmission** | Six-speed manual (6MT) | Seven-speed dual clutch (DCT7) | |
| **Acceleration (0-100 km/h) (secs)** | 10.4 | 11.1 (provisional) | |
| **Maximum speed (km/h)** | 180 | 180 | |
| **Wheels/tyres** | * 16 inch steel - 215/65 (standard on Visia grade) * 17 inch alloy – 215/60 (standard from Acenta) * 19 inch alloy – 225/45 (optional on Tekna ) | | |
| **Front suspension** | Macpherson Strut type | | |
| **Rear suspension** | Twist beam, coil spring type | | |
| **Brakes front/rear** | Disc, 280 mm / Disc, 260 mm (from N-Connecta)  w/ ABS, BA, EBD, TCS, VDC | | |
| **Exterior dimensions (mm)** | * Length: 4,210 * Width: 1,800 * Height: 1,595 * Wheelbase: 2,636 | | |
| **Rear cabin dimensions (mm)** | * Rear knee room: 583 * Rear head room: 22 * Rear shoulder room: 1,320.3 | | |
| **Luggage space capacity and dimensions** | * Max. boot aperture width (mm): 1,072 * Base boot aperture width (mm): 1,003 * Luggage capacity (l): 422 | | |
| **Min. kerb weight**  **(N-Connecta) (kg)** | 1,192 (provisional) | | 1,210 (provisional) |
| **Infotainment and connectivity** | * NissanConnect in-car infotainment system with 8 inch touch screen display (standard on Acenta, N-Connecta, Tekna)   + Apple® CarPlay, Android® Auto\* * NissanConnect Services (option on Acenta, N-Connecta, Tekna)   + Nissan on Google Assistant\*   + In-Car WiFI\*\*\*   + Driving History & Analysis\*   + Maps & Live Traffic\*\*   + Nissan Help & Support\*   + Breakdown Call\*   + Vehicle Health\*   + Smart Alerts\*\* * Colour TFT screen (4.2 inch standard on Visia, Acenta, 7 inch standard on N-Connecta, Tekna) * BOSE® Personal® Plus sound system (option from N-Connecta)   + Eight speakers, including UltraNearFIeld headrest speakers for driver and front passenger | | |
| **Safety features** | * Standard on all grades safety functionalities   + Emergency Call\*   + Cruise Control & Speed Limiter   + Intelligent Emergency Braking  with Pedestrian & Cyclist Recognition   + Intelligent Lane Intervention and Warning   + High Beam Assist   + Traffic Sign Recognition linked to Cruise Control   + Hill Start Assist * Intelligent Cruise Control (standard on Tekna; option on N-Connecta ) * Nissan ProPILOT (standard on Tekna; option on N-Connecta) * Around View Monitor (standard on Tekna; option on N-Connecta) * Intelligent Driver Alertness (standard on Tekna; option on N-Connecta) * Blind Spot Intervention (standard on Tekna; option on N-Connecta) * Rear Cross-Traffic Alert (standard on Tekna; option on N-Connecta) | | |
| **Seating capacity** | 5 | | |
| **Warranty** | 3 years / 100,000 km | | |

**\* Free for seven years, then pay per use. Availability depending on your country or region.**

**\*\* Free for three years, then pay per use. Availability depending on your country or region.**

**\*\*\* Paid only Availability depending on your country or region.**

**1 Over Torque function provides an additional 20 Nm for 25 seconds upon application of full throttle. The function is applied from second gear through to the longest gear.**

**2 19 inch standard application on Tekna according to country**